CAN messages
+ -

|  | Name | CAN ID | Type | DLC | Comment
--- | --- | --- | --- | --- | --- | ---

CAN signals ()
+ -

|  | Name | Type | Order | Mode | Multiplexor | Multiplex value | Start | Length | Factor | Offset | Min | Max | Unit | Comment
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---

CAN signal preview
Byte number

| Editor bit indices
--- | ---
| 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

| CAN frame | Bit data values
--- | --- | ---
| Data (HEX) | Data (BIN) | 7 | 6 | 5 | 4 | 3 | 2 | 1 | 0

Signal mask (BIN)
7 | 6 | 5 | 4 | 3 | 2 | 1 | 0
--- | --- | --- | --- | --- | --- | --- | ---

Signal preview only supported for bit lengths < 54 bits
Data = 0b = 0x =
Physical value = * + =
DBC preview ()

x